|  |  |  |  |
| --- | --- | --- | --- |
| Name | Unit | Evaluated Value | Description |
| Lp | mm | 5.78mm | Patch length |
| Wp | mm | 7.54mm | Patch width |
| hs | mm | 0.406mm | Substrate height |
| Ws | - | 11.736mm | Ground plane width |
| Ls | - | 18.206mm | Ground plane length |
| xfeed | mm | 1.1mm | Feed point x-offset |
| dp | mm | 3.5mm | Patch offset parameter |
| rcoax | mm | 0.16mm | Coaxial feed radius |
| hcoax | mm | 0.203mm | Coaxial feed height |
| rprope | mm | 0.07mm | Probe radius |
| yfeed | mm | 0mm | Feed point y-offset |
| hgnd | mm | -0.032mm | Ground plane height |
| Xcoax | - | 2 | Coaxial feed x-offset |
| WTL\_In | mm | 0.673367mm | Input transmission line width |
| LTL\_feed | mm | 2.179292mm | Feed transmission line length |
| WTL\_feed | mm | 0.976256mm | Feed transmission line width |
| LTL\_Slot | mm | 0.25mm | Slot length |