|  |  |  |  |
| --- | --- | --- | --- |
| Name | Unit | "Evaluated Value" | Description |
| Lp | mm | 3.633mm | Patch length |
| Wp | mm | 5.173mm | Patch width |
| hs | mm | 0.406mm | Substrate height |
| Ws | mm | 7.609mm | Ground plane width |
| Ls | mm | 10.658mm | Ground plane length |
| xsub | mm | -5.329mm | Substrate center x-offset |
| ysub | mm | -3.8045mm | Substrate center y-offset |
| xfeed | mm | 1.2mm | Feed point x-offset |
| dp | mm | 0.55mm | Patch offset parameter |
| rcoax | mm | 0.16mm | Coaxial feed radius |
| hcoax | mm | 0.203mm | Coaxial feed height |
| rprope | mm | 0.07mm | Probe radius |
| Lair | mm | 20.658mm | Airbox length |
| Wair | mm | 17.609mm | Airbox width |
| xair | mm | 10.329mm | Airbox x-center offset |
| yair | mm | 8.8045mm | Airbox y-center offset |
| hair | mm | 5mm | Airbox height |
| yfeed | mm | 0mm | Feed point y-offset |
| xp | mm | 0.275mm | Patch x-origin |
| yp | mm | -2.5865mm | Patch y-origin |
| hgnd | mm | -0.032mm | Ground plane height |